[RU] Перед обновлением устройство необходимо включить в режиме радио.

Чтобы проверить актуальность версии, необходимо по порядку нажать клавиши 615243.
Версия прошивки состоит из 8 цифр, которые должны совпадать с цифрами в конце названия файла обновления.

1. Файл обновления необходимо перенести на флеш-карту объёмом не более 16 ГБ и файловой системой FAT32;
2. Включите устройство в режиме радио, вставьте флеш-карту в соответствующий (не для зарядки) разъём;
3. Дождитесь появления оповещения об обновлении, после чего устройство должно самостоятельно полностью выключиться.
4. Извлеките флеш-карту из разъёма, включите устройство и в режиме радио проверьте актуальность версии;
5. Готово, устройством можно пользоваться в обычном режиме!

Мобильные приложение для настройки и управления устройствами серий DB-100/300DSP/500DSP доступны по ссылкам:
App Store: https://apps.apple.com/ru/app/deaf-bonce-audio-dsp/id6720728414?l=ru
Google Play: https://play.google.com/store/apps/details?id=com.db.deaf_bonce_application

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

[EN] Before updating, the unit should be turned on in the radio mode.

To check the version, please, press keys 615243 in order.
The firmware version has 8 digits, which must match the digits at the end of the update file name.

1. The update file must be moved to a flash card with a volume of not more than 16 GB and FAT32 file system;
2. Turn on the unit in radio mode, insert the flash card into the correct (not for charging) connector;
3. Wait for the update notification to appear, and then the unit should turn off completely by itself.
4. Remove the flash card from the connector, turn on the unit in radio mode and check if the version is up to date;
5. Done!

Mobile apps for setup and control of DB-100/300DSP/500DSP series untis are available below:
App Store: https://apps.apple.com/ru/app/deaf-bonce-audio-dsp/id6720728414?l=ru
Google Play: https://play.google.com/store/apps/details?id=com.db.deaf_bonce_application